Author: Hewlett Packard Enterprise

Attachment A

Open Land Required: 6.1 Acres
Open Land Provided: 8.8 Acres

Safety Zone Area Impacted by Project
Safety Zone 2: 33.81 Acres
Safety Zone 4: 87.95 Acres

Open Land Required Calculation
Safety Zone 2: x=(34 acres/10 acres) x 0.5 acres = 1.7 Acres
Safety Zone 4: x = (87.95 acres/10 acres x 0.5 acres = 4.4 Acres
Total: 6.1 Acres

Open Land Provided Calculation
Old Highway 80 in Safety Zone 4 = 5.28 Acres
Area with no development proposed with no slope = 3.52 Acres
Total: 8.8 Acres